|  |  |
| --- | --- |
| Arduino | App |
| * Receive/Send Socket commands * Read sensors and send those to the app if asked for it * On receiving the command to do so change the state of the corresponding switch | * Receive/Send Socket commands * Ask for sensor readings and process these. * Send command to Arduino to toggle a switch * Set timer to toggle a switch * Set threshold for sensor value to toggle switch |